{"text_format":"3","workbook":"xlsx","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"defined_names":1},"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":36,"n_cols":5,"rows_kept":36,"merged":[[0,0,0,4],[1,1,1,2],[2,1,2,2],[3,1,3,2],[4,1,4,2],[5,1,5,2],[6,1,6,2],[7,1,7,2],[8,1,8,2],[9,1,9,2],[10,1,10,2],[11,1,11,2],[12,1,12,2],[13,1,13,2],[14,1,14,2],[15,0,17,0],[15,1,17,1],[18,1,18,2],[19,1,19,2],[20,1,20,2],[21,1,21,2],[22,1,22,2],[23,1,23,2],[24,1,24,2],[25,1,25,2],[26,1,26,2],[27,1,27,2],[28,1,28,2],[29,1,29,2],[30,1,30,2],[31,1,31,2],[32,1,32,2],[33,1,33,2],[34,1,34,2],[35,1,35,2]]}
["连云区2025年监督抽查和风险监测产品质量抽检计划"]
["序号","产品名称",null,"检测项目","批次数"]
[1," 老年健步鞋",null,"鞋号、产品标识、感官质量、外底耐磨性能、成鞋耐折性能",1]
[2," 童鞋（旅游鞋、皮鞋、凉鞋）",null,"鞋号、产品标识、感官质量、外底耐磨性能、成鞋耐折性能",1]
[3," 学习用品（修正液/带、橡皮）",null,"可迁移元素",1]
[4," 学习用品（彩笔）",null,"笔套安全、可迁移元素",2]
[5," 学习用品（彩泥）",null,"可迁移元素",2]
[6," 学习用品（学生书袋）",null,"摩擦色牢度(沾色)、可迁移元素",2]
[7," 学习用品（文具盒、袋）",null,"可迁移元素",2]
[8," 挂烫机",null,"标志和说明、对触及带电部件的防护、输入功率和电流、工作温度下的泄漏电流和电气强度、耐潮湿、泄漏电流和电气强度、稳定性和机械危险、机械强度、结构、内部布线、电源连接和外部软线、外部导线用接线端子、接地措施、螺钉和连接、电气间隙、爬电距离和固体绝缘",1]
[9," 电热垫",null,"标志和说明、对触及带电部件的防护、输入功率和电流、发热、工作温度下的泄漏电流和电气强度、耐潮湿、泄漏电流和电气强度、非正常工作、机械强度、结构、内部布线、电源连接和外部软线、外部导线用接线端子、接地措施、螺钉和连接、电气间隙、爬电距离和固体绝缘",1]
[10," 室内加热器",null,"标志和说明、对触及带电部件的防护、输入功率和电流、工作温度下的泄漏电流和电气强度、耐潮湿、泄漏电流和电气强度、稳定性和机械危险、机械强度、结构、内部布线、电源连接和外部软线、外部导线用接线端子、接地措施、螺钉和连接、电气间隙、爬电距离和固体绝缘",1]
[11," 移动电源",null,"常温下的有效输出容量、转换效率、短路保护、碰撞、自由跌落、无线电骚扰",1]
[12," 带USB接口插座",null,"尺寸检查、防触电保护、接地措施、固定式插座的结构、插头和移动式插座的结构、防潮、绝缘电阻和电气强度、拔出插头所需的力、软缆及其连接、电气间隙、爬电距离和通过密封胶的距离、耐热、绝缘材料的耐排正常热、耐燃、外部导线用接线端子、接地措施、螺钉和连接、电气间隙、爬电距离和固体绝缘、耐热和耐燃",1]
[13," 婴幼儿纸尿裤",null,"渗透性能、微生物",2]
[14," 危险化学品"," 高纯氢氧化钠","外观、氢氧化钠、碳酸钠、氯化钠、三氧化二铁、二氧化硅、氯酸钠、硫酸钠、三氧化二铝、氧化钙",1]
[null,null," 副产盐酸","外观、总酸度、重金属、浊度",1]
[null,null," 工业用对苯二酚","外观、对苯二酚、邻苯二酚、终熔点、灼烧残渣、重金属、铁（以Fe计）、溶解性试验",1]
[15," 开关插座",null,"尺寸检查、防触电保护、接地措施、固定式插座的结构、插头和移动式插座的结构、防潮、绝缘电阻和电气强度、拔出插头所需的力、软缆及其连接、电气间隙、爬电距离和通过密封胶的距离、耐热、绝缘材料的耐排正常热、耐燃、外部导线用接线端子、接地措施、螺钉和连接、电气间隙、爬电距离和固体绝缘、耐热和耐燃",2]
[16," 珠宝玉石",null,"质量、密度、折射率、双折射率、吸收光谱、光性特征、多色性、放大检查、紫外荧光、镶嵌贵金属材质及含量",3]
[17," 热轧带肋钢筋",null,"力学性能，化学成分，重量偏差",1]
[18," 水泥",null,"安定性、凝结时间、强度",2]
[19," 预拌混凝土",null,"强度",2]
[20," 建筑用外墙涂料",null,"VOC含量、甲醛、苯系物总和含量[限苯、甲苯、二甲苯（含乙苯）]、对比率、耐洗刷性",1]
[21," 合成树脂乳液内墙涂料",null,"VOC含量、甲醛、苯系物总和含量[限苯、甲苯、二甲苯（含乙苯）]、对比率、耐洗刷性",1]
[22," 陶瓷片密封水嘴",null,"水压，螺纹精度",2]
[23," 胶粘剂",null,"游离甲醛、苯、甲苯+二甲苯、总挥发性有机物、压缩剪切强度 干强度、压缩剪切强度 湿强度、粘结强度、不挥发物",1]
[24," 车用尿素",null,"尿素含量、碱度、缩二脲、钙、铁、铝、钠、钾",3]
[25," 车用汽油",null,"馏程、硫含量、氧含量/甲醇含量、乙醇含量、密度",1]
[26," 发动机润滑油",null,"运动黏度、黏度指数、低温动力黏度、闪点（开口）、倾点",2]
[27," 电线电缆",null,"导体电阻、成品电缆电压试验、绝缘线芯电压试验、绝缘电阻、绝缘平均厚度、绝缘最薄处厚度、护套平均厚度、护套最薄厚度、绝缘老化前抗张强度、绝缘老化前断裂伸长率、绝缘老化后抗张强度、绝缘老化后断裂伸长率、绝缘老化前后抗张强度变化率、绝缘老化前后断裂伸长率变化率、护套老化前抗张强度、护套老化前断裂伸长率、护套老化后抗张强度、护套老化后断裂伸长率、护套老化前后抗张强度变化率、护套老化前后断裂伸长率变化率、绝缘失重试验、护套失重试验、热延伸",1]
[28," 食品接触用纸包装及容器等制品",null,"杯身挺度、抗压强度、荧光物质、甲醛、微生物指标",1]
[29," 餐具洗涤剂",null,"总活性物含量、pH、甲醛、砷、重金属",2]
[30," 手提式灭火器",null,"瓶体-爆破试验、灭火剂（干粉灭火剂）-第一主要组分含量",2]
[31," 建筑保温材料",null,"导热系数、燃烧性能",2]
["合计",{"$nulls":3},50]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0}